**Termite Risk Management Notice**

* **THIS SHOULD BE COVERED IN A DURABLE MATERIAL (PLASTIC, ETC) AND FIXED IN A PROMINENT LOCATION (METER BOX, KITCHEN CUPBOARD, ETC.) ALTERNATIVELY,**
* **THE OWNER MAY CHOOSE TO LAMINATE THE ABOVE NOTICE.**

✂

|  |  |
| --- | --- |
| **Termite Risk Management Notice**  *As per Part 3.1.3.2 of the Building Code of Australia* | |
| **1. METHOD OF TERMITE RISK MANAGEMENT:** |  |
| **2. DATE OF INSTALLATION:** |  |
| **3. LIFE EXPECTANCY (Chemical Barrier Only)** |  |
| **4. INSPECTION AND MAINTENANCE**  This Termite Protection System needs to be maintained on a regular basis. The Australian Standard for termite protection AS 3660.1 (2014) recommends regular, competent INSPECTION of the building for termite activity at least every twelve months. This is to ensure that termites have not bridged or breached the system and entered the building.  Disturbance or covering of the treated soil in contact with the building or attachments may render this structure liable to termite attack. The home owner is advised to have competent inspections to ensure the external barrier is not disturbed. Your professional pest control manager can advise on any follow-up protection required, or maintenance of your termite protection system. | |
| INSTALLER/ BUILDER: | |
| ADDRESS: | |
| TELEPHONE: | |